0.5% Grade 4.8MWH 100 Mile Corridor:

131.5 ton cars are impossible to achieve infinity train operation without charging station at the end, the battery will never fully recharge with loaded train come down. The boundary E/L weight ratio is between 131.5 ton cars and 143 ton-cars.